(kicad_sch
	(version 20250114)
	(generator "eeschema")
	(generator_version "9.0")
	(paper "A4")
	(title_block
		(title "Reversed Engineered Electrolux ErgoRapido Handle Remote PCB")
		(date "2025-08-03")
		(rev "1")
	)
	(lib_symbols
		(symbol "Connector:Conn_01x01_Pin"
			(pin_names
				(offset 1.016)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "J"
				(at 0 2.54 0)
			)
			(property "Value" "Conn_01x01_Pin"
				(at 0 -2.54 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Generic connector, single row, 01x01, script generated"
				(at 0 0 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(property "ki_keywords" "connector"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Connector*:*_1x??_*"
				(at 0 0 0)
			)
			(symbol "Conn_01x01_Pin_1_1"
				(rectangle
					(start 0.8636 0.127)
					(end 0 -0.127)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy 1.27 0) (xy 0.8636 0)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 5.08 0 180)
					(length 3.81)
					(name "Pin_1")
					(number "1")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Device:C"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0.254)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 0.635 2.54 0)
			)
			(property "Value" "C"
				(at 0.635 -2.54 0)
			)
			(property "Footprint" ""
				(at 0.9652 -3.81 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Unpolarized capacitor"
				(at 0 0 0)
			)
			(property "ki_keywords" "cap capacitor"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "C_*"
				(at 0 0 0)
			)
			(symbol "C_0_1"
				(polyline
					(pts
						(xy -2.032 0.762) (xy 2.032 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -2.032 -0.762) (xy 2.032 -0.762)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "C_1_1"
				(pin passive line
					(at 0 3.81 270)
					(length 2.794)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 2.794)
					(name "~")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Device:LED"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 1.016)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "D"
				(at 0 2.54 0)
			)
			(property "Value" "LED"
				(at 0 -2.54 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Light emitting diode"
				(at 0 0 0)
			)
			(property "Sim.Pins" "1=K 2=A"
				(at 0 0 0)
			)
			(property "ki_keywords" "LED diode"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "LED* LED_SMD:* LED_THT:*"
				(at 0 0 0)
			)
			(symbol "LED_0_1"
				(polyline
					(pts
						(xy -3.048 -0.762) (xy -4.572 -2.286) (xy -3.81 -2.286) (xy -4.572 -2.286) (xy -4.572 -1.524)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.778 -0.762) (xy -3.302 -2.286) (xy -2.54 -2.286) (xy -3.302 -2.286) (xy -3.302 -1.524)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.27 0) (xy 1.27 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.27 -1.27) (xy -1.27 1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 -1.27) (xy 1.27 1.27) (xy -1.27 0) (xy 1.27 -1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "LED_1_1"
				(pin passive line
					(at -3.81 0 0)
					(length 2.54)
					(name "K")
					(number "1")
				)
				(pin passive line
					(at 3.81 0 180)
					(length 2.54)
					(name "A")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Device:Polyfuse"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "F"
				(at -2.54 0 90)
			)
			(property "Value" "Polyfuse"
				(at 2.54 0 90)
			)
			(property "Footprint" ""
				(at 1.27 -5.08 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Resettable fuse, polymeric positive temperature coefficient"
				(at 0 0 0)
			)
			(property "ki_keywords" "resettable fuse PTC PPTC polyfuse polyswitch"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "*polyfuse* *PTC*"
				(at 0 0 0)
			)
			(symbol "Polyfuse_0_1"
				(polyline
					(pts
						(xy -1.524 2.54) (xy -1.524 1.524) (xy 1.524 -1.524) (xy 1.524 -2.54)
					)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -0.762 2.54)
					(end 0.762 -2.54)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 2.54) (xy 0 -2.54)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "Polyfuse_1_1"
				(pin passive line
					(at 0 3.81 270)
					(length 1.27)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 1.27)
					(name "~")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Device:R"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 2.032 0 90)
			)
			(property "Value" "R"
				(at 0 0 90)
			)
			(property "Footprint" ""
				(at -1.778 0 90)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Resistor"
				(at 0 0 0)
			)
			(property "ki_keywords" "R res resistor"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "R_*"
				(at 0 0 0)
			)
			(symbol "R_0_1"
				(rectangle
					(start -1.016 -2.54)
					(end 1.016 2.54)
					(fill
						(type none)
					)
				)
			)
			(symbol "R_1_1"
				(pin passive line
					(at 0 3.81 270)
					(length 1.27)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 1.27)
					(name "~")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Diode:1N4148WT"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "D"
				(at 0 2.54 0)
			)
			(property "Value" "1N4148WT"
				(at 0 -2.54 0)
			)
			(property "Footprint" "Diode_SMD:D_SOD-523"
				(at 0 -4.445 0)
			)
			(property "Datasheet" "https://www.diodes.com/assets/Datasheets/ds30396.pdf"
				(at 0 0 0)
			)
			(property "Description" "75V 0.15A Fast switching Diode, SOD-523"
				(at 0 0 0)
			)
			(property "Sim.Device" "D"
				(at 0 0 0)
			)
			(property "Sim.Pins" "1=K 2=A"
				(at 0 0 0)
			)
			(property "ki_keywords" "diode"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "D*SOD?523*"
				(at 0 0 0)
			)
			(symbol "1N4148WT_0_1"
				(polyline
					(pts
						(xy -1.27 1.27) (xy -1.27 -1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 1.27) (xy 1.27 -1.27) (xy -1.27 0) (xy 1.27 1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 0) (xy -1.27 0)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "1N4148WT_1_1"
				(pin passive line
					(at -3.81 0 0)
					(length 2.54)
					(name "K")
					(number "1")
				)
				(pin passive line
					(at 3.81 0 180)
					(length 2.54)
					(name "A")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Switch:SW_Push"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 1.016)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "SW"
				(at 1.27 2.54 0)
			)
			(property "Value" "SW_Push"
				(at 0 -1.524 0)
			)
			(property "Footprint" ""
				(at 0 5.08 0)
			)
			(property "Datasheet" "~"
				(at 0 5.08 0)
			)
			(property "Description" "Push button switch, generic, two pins"
				(at 0 0 0)
			)
			(property "ki_keywords" "switch normally-open pushbutton push-button"
				(at 0 0 0)
			)
			(symbol "SW_Push_0_1"
				(circle
					(center -2.032 0)
					(radius 0.508)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 1.27) (xy 0 3.048)
					)
					(fill
						(type none)
					)
				)
				(circle
					(center 2.032 0)
					(radius 0.508)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.54 1.27) (xy -2.54 1.27)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at -5.08 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 5.08 0 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Transistor_BJT:BC817"
			(pin_names
				(offset 0)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "Q"
				(at 5.08 1.905 0)
			)
			(property "Value" "BC817"
				(at 5.08 0 0)
			)
			(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
				(at 5.08 -1.905 0)
			)
			(property "Datasheet" "https://www.onsemi.com/pub/Collateral/BC818-D.pdf"
				(at 0 0 0)
			)
			(property "Description" "0.8A Ic, 45V Vce, NPN Transistor, SOT-23"
				(at 0 0 0)
			)
			(property "ki_keywords" "NPN Transistor"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "SOT?23*"
				(at 0 0 0)
			)
			(symbol "BC817_0_1"
				(polyline
					(pts
						(xy -2.54 0) (xy 0.635 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.635 1.905) (xy 0.635 -1.905)
					)
					(fill
						(type none)
					)
				)
				(circle
					(center 1.27 0)
					(radius 2.8194)
					(fill
						(type none)
					)
				)
			)
			(symbol "BC817_1_1"
				(polyline
					(pts
						(xy 0.635 0.635) (xy 2.54 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.635 -0.635) (xy 2.54 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 -1.778) (xy 1.778 -1.27) (xy 2.286 -2.286) (xy 1.27 -1.778)
					)
					(fill
						(type outline)
					)
				)
				(pin input line
					(at -5.08 0 0)
					(length 2.54)
					(name "B")
					(number "1")
				)
				(pin passive line
					(at 2.54 5.08 270)
					(length 2.54)
					(name "C")
					(number "3")
				)
				(pin passive line
					(at 2.54 -5.08 90)
					(length 2.54)
					(name "E")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
	)
	(rectangle
		(start 17.78 24.13)
		(end 275.59 161.29)
		(fill
			(type none)
		)
	)
	(rectangle
		(start 21.59 88.9)
		(end 271.78 157.48)
		(fill
			(type none)
		)
	)
	(text "CHARGING INDICATOR"
		(exclude_from_sim no)
		(at 154.686 46.228 0)
	)
	(text "SW2 is Power Up/Down Toggle"
		(exclude_from_sim no)
		(at 228.092 100.838 0)
	)
	(text "Debounce?"
		(exclude_from_sim no)
		(at 86.868 133.35 0)
	)
	(text "SW2 is Power On/Off Toggle"
		(exclude_from_sim no)
		(at 228.346 127.762 0)
	)
	(text "Electrolux ErgoRapido ZB3012\nElectrolux ErgoRapido ZB3004\n"
		(exclude_from_sim no)
		(at 41.656 94.742 0)
	)
	(text "Reversed Engineered Handle Switch PCB\nBy Brian Khuu 2025\nFor Electrolux ErgoRapido (ZB3012)\nElectrolux 2012 / 1183813 R4\n"
		(exclude_from_sim no)
		(at 179.578 173.228 0)
	)
	(text "Electrolux ErgoRapido ZB3004"
		(exclude_from_sim no)
		(at 251.206 35.814 0)
	)
	(junction
		(at 190.5 114.3)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 88.9 50.8)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 60.96 38.1)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 266.7 139.7)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 177.8 114.3)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 72.39 114.3)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 88.9 76.2)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 72.39 152.4)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 115.57 50.8)
		(diameter 0)
		(color 0 0 0 0)
	)
	(wire
		(pts
			(xy 266.7 152.4) (xy 72.39 152.4)
		)
	)
	(wire
		(pts
			(xy 106.68 50.8) (xy 115.57 50.8)
		)
	)
	(wire
		(pts
			(xy 166.37 38.1) (xy 177.8 38.1)
		)
	)
	(wire
		(pts
			(xy 266.7 114.3) (xy 266.7 139.7)
		)
	)
	(wire
		(pts
			(xy 106.68 76.2) (xy 134.62 76.2)
		)
	)
	(wire
		(pts
			(xy 88.9 50.8) (xy 88.9 76.2)
		)
	)
	(wire
		(pts
			(xy 60.96 38.1) (xy 115.57 38.1)
		)
	)
	(wire
		(pts
			(xy 134.62 55.88) (xy 134.62 76.2)
		)
	)
	(wire
		(pts
			(xy 38.1 152.4) (xy 72.39 152.4)
		)
	)
	(wire
		(pts
			(xy 266.7 139.7) (xy 266.7 152.4)
		)
	)
	(wire
		(pts
			(xy 190.5 114.3) (xy 210.82 114.3)
		)
	)
	(wire
		(pts
			(xy 72.39 114.3) (xy 72.39 129.54)
		)
	)
	(wire
		(pts
			(xy 72.39 152.4) (xy 72.39 137.16)
		)
	)
	(wire
		(pts
			(xy 115.57 50.8) (xy 127 50.8)
		)
	)
	(wire
		(pts
			(xy 99.06 76.2) (xy 88.9 76.2)
		)
	)
	(wire
		(pts
			(xy 210.82 139.7) (xy 190.5 139.7)
		)
	)
	(wire
		(pts
			(xy 72.39 114.3) (xy 177.8 114.3)
		)
	)
	(wire
		(pts
			(xy 190.5 139.7) (xy 190.5 114.3)
		)
	)
	(wire
		(pts
			(xy 77.47 50.8) (xy 88.9 50.8)
		)
	)
	(wire
		(pts
			(xy 88.9 50.8) (xy 99.06 50.8)
		)
	)
	(wire
		(pts
			(xy 220.98 114.3) (xy 237.49 114.3)
		)
	)
	(wire
		(pts
			(xy 220.98 139.7) (xy 237.49 139.7)
		)
	)
	(wire
		(pts
			(xy 134.62 38.1) (xy 134.62 45.72)
		)
	)
	(wire
		(pts
			(xy 245.11 139.7) (xy 266.7 139.7)
		)
	)
	(wire
		(pts
			(xy 177.8 38.1) (xy 177.8 114.3)
		)
	)
	(wire
		(pts
			(xy 60.96 50.8) (xy 60.96 38.1)
		)
	)
	(wire
		(pts
			(xy 115.57 38.1) (xy 115.57 50.8)
		)
	)
	(wire
		(pts
			(xy 69.85 50.8) (xy 60.96 50.8)
		)
	)
	(wire
		(pts
			(xy 78.74 76.2) (xy 88.9 76.2)
		)
	)
	(wire
		(pts
			(xy 38.1 76.2) (xy 71.12 76.2)
		)
	)
	(wire
		(pts
			(xy 38.1 38.1) (xy 60.96 38.1)
		)
	)
	(wire
		(pts
			(xy 151.13 38.1) (xy 158.75 38.1)
		)
	)
	(wire
		(pts
			(xy 245.11 114.3) (xy 266.7 114.3)
		)
	)
	(wire
		(pts
			(xy 177.8 114.3) (xy 190.5 114.3)
		)
	)
	(wire
		(pts
			(xy 72.39 114.3) (xy 38.1 114.3)
		)
	)
	(wire
		(pts
			(xy 134.62 38.1) (xy 143.51 38.1)
		)
	)
	(label "BUTTON_SENSE"
		(at 45.72 152.4 0)
	)
	(label "BATTERY_OUTPUT"
		(at 45.72 114.3 0)
	)
	(label "PWR_INPUT"
		(at 45.72 38.1 0)
	)
	(label "BATTERY_CHARGE_INPUT"
		(at 46.99 76.2 0)
	)
	(symbol
		(lib_id "Device:C")
		(at 72.39 133.35 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C1"
			(at 76.2 132.0799 0)
		)
		(property "Value" "C?"
			(at 76.2 134.6199 0)
		)
		(property "Footprint" ""
			(at 73.3552 137.16 0)
		)
		(property "Datasheet" "~"
			(at 72.39 133.35 0)
		)
		(property "Description" "Unpolarized capacitor"
			(at 72.39 133.35 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project ""
				(path
					(reference "C1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Connector:Conn_01x01_Pin")
		(at 33.02 114.3 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "J3"
			(at 33.655 109.22 0)
		)
		(property "Value" "Conn_01x01_Pin"
			(at 33.655 111.76 0)
		)
		(property "Footprint" "Connector_Wire:SolderWire-0.1sqmm_1x01_D0.4mm_OD1mm"
			(at 33.02 114.3 0)
		)
		(property "Datasheet" "~"
			(at 33.02 114.3 0)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated"
			(at 33.02 114.3 0)
		)
		(pin "1")
		(instances
			(project "Electrolux ErgoRapido ZB3012"
				(path
					(reference "J3")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 241.3 139.7 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R4"
			(at 241.3 133.35 90)
		)
		(property "Value" "4.7k"
			(at 241.3 135.89 90)
		)
		(property "Footprint" ""
			(at 241.3 137.922 90)
		)
		(property "Datasheet" "~"
			(at 241.3 139.7 0)
		)
		(property "Description" "Resistor"
			(at 241.3 139.7 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Electrolux ErgoRapido ZB3012"
				(path
					(reference "R4")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 241.3 114.3 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R3"
			(at 241.3 107.95 90)
		)
		(property "Value" "1k"
			(at 241.3 110.49 90)
		)
		(property "Footprint" ""
			(at 241.3 112.522 90)
		)
		(property "Datasheet" "~"
			(at 241.3 114.3 0)
		)
		(property "Description" "Resistor"
			(at 241.3 114.3 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Electrolux ErgoRapido ZB3012"
				(path
					(reference "R3")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Switch:SW_Push")
		(at 215.9 114.3 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "SW1"
			(at 215.9 106.68 0)
		)
		(property "Value" "SW_Push"
			(at 215.9 109.22 0)
		)
		(property "Footprint" ""
			(at 215.9 109.22 0)
		)
		(property "Datasheet" "~"
			(at 215.9 109.22 0)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 215.9 114.3 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project ""
				(path
					(reference "SW1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Transistor_BJT:BC817")
		(at 132.08 50.8 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "Q1"
			(at 140.97 50.8 90)
		)
		(property "Value" "BC817 ?"
			(at 138.43 50.8 90)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 137.16 52.705 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/BC818-D.pdf"
			(at 132.08 50.8 0)
		)
		(property "Description" "0.8A Ic, 45V Vce, NPN Transistor, SOT-23"
			(at 132.08 50.8 0)
		)
		(pin "2")
		(pin "3")
		(pin "1")
		(instances
			(project "Electrolux ErgoRapido ZB3012"
				(path
					(reference "Q1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:Polyfuse")
		(at 74.93 76.2 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "F1"
			(at 73.6599 73.66 0)
		)
		(property "Value" "Polyfuse"
			(at 76.1999 73.66 0)
		)
		(property "Footprint" ""
			(at 80.01 74.93 0)
		)
		(property "Datasheet" "~"
			(at 74.93 76.2 0)
		)
		(property "Description" "Resettable fuse, polymeric positive temperature coefficient"
			(at 74.93 76.2 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "Electrolux ErgoRapido ZB3012"
				(path
					(reference "F1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 147.32 38.1 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R5"
			(at 147.32 31.75 90)
		)
		(property "Value" "250"
			(at 147.32 34.29 90)
		)
		(property "Footprint" ""
			(at 147.32 36.322 90)
		)
		(property "Datasheet" "~"
			(at 147.32 38.1 0)
		)
		(property "Description" "Resistor"
			(at 147.32 38.1 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Electrolux ErgoRapido ZB3012"
				(path
					(reference "R5")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Connector:Conn_01x01_Pin")
		(at 33.02 76.2 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "J2"
			(at 33.655 71.12 0)
		)
		(property "Value" "Conn_01x01_Pin"
			(at 33.655 73.66 0)
		)
		(property "Footprint" "Connector_Wire:SolderWire-0.1sqmm_1x01_D0.4mm_OD1mm"
			(at 33.02 76.2 0)
		)
		(property "Datasheet" "~"
			(at 33.02 76.2 0)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated"
			(at 33.02 76.2 0)
		)
		(pin "1")
		(instances
			(project "Electrolux ErgoRapido ZB3012"
				(path
					(reference "J2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Switch:SW_Push")
		(at 215.9 139.7 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "SW2"
			(at 215.9 132.08 0)
		)
		(property "Value" "SW_Push"
			(at 215.9 134.62 0)
		)
		(property "Footprint" ""
			(at 215.9 134.62 0)
		)
		(property "Datasheet" "~"
			(at 215.9 134.62 0)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 215.9 139.7 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Electrolux ErgoRapido ZB3012"
				(path
					(reference "SW2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 102.87 76.2 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R1"
			(at 102.87 69.85 90)
		)
		(property "Value" "33"
			(at 102.87 72.39 90)
		)
		(property "Footprint" ""
			(at 102.87 74.422 90)
		)
		(property "Datasheet" "~"
			(at 102.87 76.2 0)
		)
		(property "Description" "Resistor"
			(at 102.87 76.2 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Electrolux ErgoRapido ZB3012"
				(path
					(reference "R1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Connector:Conn_01x01_Pin")
		(at 33.02 152.4 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "J4"
			(at 33.655 147.32 0)
		)
		(property "Value" "Conn_01x01_Pin"
			(at 33.655 149.86 0)
		)
		(property "Footprint" "Connector_Wire:SolderWire-0.1sqmm_1x01_D0.4mm_OD1mm"
			(at 33.02 152.4 0)
		)
		(property "Datasheet" "~"
			(at 33.02 152.4 0)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated"
			(at 33.02 152.4 0)
		)
		(pin "1")
		(instances
			(project "Electrolux ErgoRapido ZB3012"
				(path
					(reference "J4")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 102.87 50.8 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R2"
			(at 102.87 44.45 90)
		)
		(property "Value" "22"
			(at 102.87 46.99 90)
		)
		(property "Footprint" ""
			(at 102.87 49.022 90)
		)
		(property "Datasheet" "~"
			(at 102.87 50.8 0)
		)
		(property "Description" "Resistor"
			(at 102.87 50.8 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Electrolux ErgoRapido ZB3012"
				(path
					(reference "R2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:LED")
		(at 162.56 38.1 0)
		(mirror x)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "L1"
			(at 160.9725 30.48 0)
		)
		(property "Value" "LED"
			(at 160.9725 33.02 0)
		)
		(property "Footprint" ""
			(at 162.56 38.1 0)
		)
		(property "Datasheet" "~"
			(at 162.56 38.1 0)
		)
		(property "Description" "Light emitting diode"
			(at 162.56 38.1 0)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 162.56 38.1 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project ""
				(path
					(reference "L1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Connector:Conn_01x01_Pin")
		(at 33.02 38.1 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "J1"
			(at 33.655 33.02 0)
		)
		(property "Value" "Conn_01x01_Pin"
			(at 33.655 35.56 0)
		)
		(property "Footprint" "Connector_Wire:SolderWire-0.1sqmm_1x01_D0.4mm_OD1mm"
			(at 33.02 38.1 0)
		)
		(property "Datasheet" "~"
			(at 33.02 38.1 0)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated"
			(at 33.02 38.1 0)
		)
		(pin "1")
		(instances
			(project ""
				(path
					(reference "J1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Diode:1N4148WT")
		(at 73.66 50.8 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D1"
			(at 73.66 44.45 0)
		)
		(property "Value" "1N4148WT"
			(at 73.66 46.99 0)
		)
		(property "Footprint" "Diode_SMD:D_SOD-523"
			(at 73.66 46.355 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/ds30396.pdf"
			(at 73.66 50.8 0)
		)
		(property "Description" "75V 0.15A Fast switching Diode, SOD-523"
			(at 73.66 50.8 0)
		)
		(property "Sim.Device" "D"
			(at 73.66 50.8 0)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 73.66 50.8 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project ""
				(path
					(reference "D1")
					(unit 1)
				)
			)
		)
	)
	(sheet_instances
		(path
			(page "1")
		)
	)
	(embedded_fonts no)
)
